California State University Los Angeles

ENVIRONMENTAL HEALTH AND SAFETY

Formulario de inspección anual de escaleras

APPENDIX 9.1

|  |  |
| --- | --- |
| **Department or Shop:**  | **Date of Inspection:**  |
| **Inspected By:**  |
| **Ladder Location (Building/Room, Shop, Cart, or Truck):**  |
| **INSPECTION ITEMS**  | OK | Needs Repair | N/A |
|  |  |  |  |
| **STEP LADDERS**  |  |  |  |
| Manufacturer’s labels present and legible  |  |  |  |
| Wobble (from loose joints)  |  |  |  |
| Damaged or worn non-slip bases |  |  |  |
| Strained, bent, split or broken braces, rungs or steps  |  |  |  |
| Rungs or steps are free of obstacles, grease, oil, or dirt  |  |  |  |
| Rungs or steps are slip resistant (knurled, corrugated)  |  |  |  |
| Loose or bent hinge spreaders  |  |  |  |
| Broken stop on hinge spreaders  |  |  |  |
| Wood surface coat transparent allowing visual inspection |  |  |  |
| **EXTENSION LADDERS**  |  |  |  |
| Manufacturer’s labels present and legible  |  |  |  |
| Damaged or worn ladder feet  |  |  |  |
| Bent, cracked, split, or broken braces, rungs, or uprights  |  |  |  |
| Rungs or steps are free of grease, oil, dirt, and slip resistant  |  |  |  |
| Loose, broken or missing extension locks  |  |  |  |
| Defective locks that do not seat properly when ladder is extended  |  |  |  |
| Frayed or worn rope  |  |  |  |
| **FIXED LADDERS**  |  |  |  |
| Loose rungs, steps, or metal fasteners (can be moved by hand)  |  |  |  |
| Bent, cracked, split or broken uprights, braces, rungs or steps  |  |  |  |
| Damaged or worn non-slip bases  |  |  |  |
| Rungs/steps missing  |  |  |  |
| **PORTABLE WHEELED LADDERS**  |  |  |  |
| Broken stop on wheel  |  |  |  |
| Bent, cracked, split or broken rails, braces, rungs, or steps  |  |  |  |
| Loose rungs or steps, nails, screws, bolts, or other parts  |  |  |  |
| Broken wheel(s)  |  |  |  |

Remember:

Ladders that are unable to be repaired must be effectively rendered unusable prior to disposal.

California State University Los Angeles

SEGURIDAD Y SALUD AMBIENTAL

Formulario de inspección anual de escaleras

APÉNDICE 9.1

|  |  |
| --- | --- |
| **Departamento o tienda:**  | **Fecha de inspección:**  |
| **Inspeccionado por:**  |
| **Ubicación de la escalera (edificio/sala, tienda, carro o camión):**  |
| **ELEMENTOS DE INSPECCIÓN**  | Vale | Necesita reparación | N / A |
|  |   |   |   |
| **ESCALERAS**  |   |   |   |
| Fabricante etiquetas presente y legible  |   |   |   |
| Bamboleo (de uniones flojas)  |   |   |   |
| Bases antideslizantes dañados o desgastados |   |   |   |
| Estirado, doblada, fractura o llaves rotas o peldaños  |   |   |   |
| Peldaños o pasos estén libres de obstáculos, grasa, aceite o suciedad  |   |   |   |
| O peldaños son antideslizantes (estriado, corrugado)  |   |   |   |
| Esparcidores de bisagras flojas o dobladas  |   |   |   |
| Parada roto en separadores de bisagra  |   |   |   |
| Madera capa superficial transparente que permite la inspección visual |   |   |   |
| **ESCALERAS DE EXTENSIÓN**  |   |   |   |
| Fabricante etiquetas presente y legible  |   |   |   |
| Pies de la escalera dañados o desgastados  |   |   |   |
| Doblado, agrietados, fractura o fracturas apoyos, peldaños o montantes  |   |   |   |
| O peldaños son libre de grasa, aceite, suciedad, antideslizante y resistente a  |   |   |   |
| Cerraduras de extensión sueltos, rotos o ausentes  |   |   |   |
| Cerraduras defectuosas que no asienta bien cuando la escalera se extiende  |   |   |   |
| Deshilachado o desgastada  |   |   |   |
| **ESCALERAS FIJAS**  |   |   |   |
| Los sujetadores de metal (puede ser movido a mano), pasos o peldaños flojos  |   |   |   |
| Doblado, agrietado, split o columnas rotas, abrazaderas o peldaños  |   |   |   |
| Bases antideslizantes dañados o desgastados  |   |   |   |
| Peldaños, escalones que faltan  |   |   |   |
| **TRASLADABLES CON RUEDAS**  |   |   |   |
| Quebrada parada en rueda  |   |   |   |
| Doblado, agrietado, split o rieles rotos, llaves, peldaños o pasos  |   |   |   |
| Peldaños flojos o pasos, clavos, tornillos, pernos u otras piezas  |   |   |   |
| Ruedas rotas  |   |   |   |

Recuerde:

Escaleras que son incapaces de ser reparado deben ser efectivamente prestados inutilizables antes de la eliminación.